HEADING/LINK 22 SEGMENT

PERIOD/090001ZSEP2019/212359ZSEP2019/

GENTEXT/JICC DATA/LINK 22 MANAGER WILL BE LOCATED AT JICC LOCATED AT OSBOURNE HEAD. CS SKYNET. POC PO1 JIMMO. TEL 902-453-1234//

NSNET/EXERCISE CUTLASS FURY 19/00010/00011/090001ZSEP2019/2/8/10//

JCRYPDAT/12/WKRP1234A/WKRP12340A1/01/23//

FORCEFLTR/-//

NNET/1/01001/00010/00011/SNC/DTDMA:ENABLED/DIVS: DISABLED//

NNET/2/02002/00010/00011/DLP/DTDMA:ENABLED/DIVS: DISABLED//

NNETPART/00010/00011/00012/00013/00014/00016/00025/00027//

NNMEPARS/UHFEPM/1/-/-/-/A12E0AA/PROBING/NST: 090001ZSEP2019-/ PST:1212359ZSEP2019/UHFEPM1//

NNMEPARS/HFFF/2/1234MHZ/4321MHZ/-/-/SHORT/ NST: 090001ZSEP2019-/ PST:1212359ZSEP2019/HFFF6//

NNCS/256/00010/16/00011/16/00012/32/00013/32/00014/16/00016/16/00025/2/00027/2//

NUBWR/75/0/00010/4/1/00011/4/1/00012/7/1/00013/7/1/00014/4/1/00016/14/1/00025/2/1/00027/2/1//

NCRYPLST/01/090001ZSEP2019//

GENTEXT/INITIALIZATION PROCEDURES/ JICC WILL DIRECT TOR AS NMU TO COMMENCE NETWORK INITIALIZATION WITH PARTICIPATANTS. ALL PARTICIPANTS WILL ENTER NETWORK IN NUMERICAL ORDER OF NU. IF AN NU UNABLE TO JOIN DURING THIS TIMEFRAME THEY MUST CONDUCT LATE JOIN PROCEDURE//

NMASN/-/-/-/-//

FORCEFLTR/FAB28/FAB32//

NUDATA/SHIP:TORONTO/UIC:CANN1238/CS:TORONTO/00010/06100-06177/1/ACTIVE/ACTIVE/10/-//

LKDUTY/840/843/845S//

NUDATA/SHIP:MONTREAL/UIC:CANN1240/CS:MONTREAL/00011/05600-05677/1/ACTIVE/ACTIVE/10/-//

LKDUTY/840S/843S/845//

NUDATA/SHIP:FREDERICTON/UIC:CANN1234/CS:FREDDY/00012/05000-05077/1/ACTIVE/ DISABLED/-/06600-06777//

LKDUTY/841S/844//

NUDATA/SHIP:HALIFAX/UIC:CANN1237/CS:HALIFAX/00013/05300-05377/1/ACTIVE/ DISABLED/-/06200-06277//

LKDUTY/841/844S//

NUDATA/SHIP:STJOHNS/UIC:CANN1235/CS:STJOHNS/00014/05200-05277/1/ACTIVE/DISABLED/-//

LKDUTY/-//

NUDATA/SHIP:VILLEDEQUEBEC/UIC:CANN1236/CS:VDQ/00016/05400-05477/1/ACTIVE/DISABLED/-/-//

LKDUTY/-//

NUDATA/UNIT:12ER/UIC:CANF0010/CS:12ER/00025/04500-04547/1 /ACTIVE/DISABLED/-/-//

LKDUTY/-//

NUDATA/UNIT:MLSCE/UIC:CANN1245/CS:MLSCE/00027/04700-04717/1/ACTIVE/ DISABLED/-/-//

NULRQ/1/00010/3//

NUNNRS/2//

UNITFLTR/-//

GENTEXT/MISSION AREA SUMMARY/JOINT EXERCISE WILL OPERATE WITHIN 50NM OFF EAST COAST OF HALIFAX NS. ALL OPAREAS IAW EXDIR CUTLASS FURY 19//

GENTEXT/LATE NETWORK INSTRUCTIONS/ALL NU REQUIREING LATE NET ENTRY ARE TO FIRST CONTACT SKYNET IN JICC FOR AUTHORIZATION. LATE NET ENTRY UNIT WILL BE MON, WITH TOR AS BACKUP. //

GENTEXT/L22 NETWORK PROCEDURES/ FRE WILL BE FNUAJ. PRIMARY RESPONSIBLE FOR DATA FORWARDING LINK22 TACTICAL PICTURE TO LINK16 NETWORKS//